Elijah Craig

This document explains how the ADCS and the IHU are communicating down to the byte by byte level.

ADCS Interface

Detailed Description of the ADCS and IHU Interface

Revision: 1.0.6



Table of Contents

[1 Hardware Layer 3](#_Toc524706749)

[2 Software Layer 4](#_Toc524706750)

[2.1 Location Data Request 4](#_Toc524706751)

[2.1.1 IHU to ADCS 4](#_Toc524706752)

[2.1.2 ADCS to IHU 4](#_Toc524706753)

[2.2 Orientation Data Request 4](#_Toc524706754)

[2.2.1 IHU to ADCS 4](#_Toc524706755)

[2.2.2 ADCS to IHU 5](#_Toc524706756)

[2.3 Temperature Data Request 5](#_Toc524706757)

[2.3.1 IHU to ADCS 5](#_Toc524706758)

[2.3.2 ADCS to IHU 5](#_Toc524706759)

[2.4 Coil Control Data Request 5](#_Toc524706760)

[2.4.1 IHU to ADCS 5](#_Toc524706761)

[2.4.2 ADCS to IHU 5](#_Toc524706762)

[2.5 Coil Current Data Request 6](#_Toc524706763)

[2.5.1 IHU to ADCS 6](#_Toc524706764)

[2.5.2 ADCS to IHU 6](#_Toc524706765)

[2.6 Orientation Commands 6](#_Toc524706766)

[2.6.1 IHU to ADCS 6](#_Toc524706767)

[2.6.2ADCS to IHU 6](#_Toc524706768)

[2.7 Satellite Maneuvers for Earth 7](#_Toc524706769)

[2.7.1 IHU to ADCS 7](#_Toc524706770)

[2.7.2 ADCS to IHU 7](#_Toc524706771)

[2.8 Satellite Maneuvers for Space 7](#_Toc524706772)

[2.8.1 IHU to ADCS 7](#_Toc524706773)

[2.8.2 ADCS to IHU 7](#_Toc524706774)

[2.9 Roast the Chicken 8](#_Toc524706775)

[2.9.1 IHU to ADCS 8](#_Toc524706776)

[2.9.2 ADCS to IHU 8](#_Toc524706777)

[2.10 Drift 8](#_Toc524706778)

[2.10.1 IHU to ADCS 8](#_Toc524706779)

[2.10.2 ADCS to IHU 8](#_Toc524706780)

[3 Example Communication 9](#_Toc524706781)

[3.1 Simple Data Request for Location 9](#_Toc524706782)

[3.2 Simple Repeated Data Request 9](#_Toc524706783)

# 1 Hardware Layer

The hardware interface between the ADCS and the IHU is I2C. It is a standard implementation of I2C with a clock wire and a data wire. See [Wikipedia’s I2C article](https://en.wikipedia.org/wiki/I%C2%B2C) for details on how it works.

# 2 Software Layer

The Attitude Determination Control System, located at 8b address 0xAC, is a slave board to the IHU. The ADCS senses and controls the satellites orientation when in orbit. The IHU will periodically request data from the ADCS to prepare an updated telemetry packet. The ADCS data will be read at 0xAD. Upon receiving multiple commands, the reading done by ADCS will reflect the most recent command. In all commands sent to ADCS, the first byte represents the command ID (CID).

## 2.1 Location Data Request

The latitude and longitude are geographic coordinates[[1]](#endnote-1), represented by 32b signed integers with 100µmin/LSB. For latitude, -90° S is represented by 0, and 90° N is represented by 232. Similarly, longitude is represented by -180° E being 0, and 180° W is 232.

### 2.1.1 IHU to ADCS

The first byte represents the command ID.

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Byte  Offset | 0x00 | 0x01 | 0x02 | 0x03 | 0x04 | 0x05 | 0x06 | 0x07 |
| 0x00 | 0x00: Location Request |  |  |  |  |  |  |  |

### 2.1.2 ADCS to IHU

The ADCS replies with an array of two geographic coordinates.

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Byte  Offset | 0x00 | 0x01 | 0x02 | 0x03 | 0x04 | 0x05 | 0x06 | 0x07 |
| 0x00 | Latitude Coordinate | | | | Longitude Coordinate | | | |

## 2.2 Orientation Data Request

Roll, Pitch, and Yaw are all angles, represented by 16b unsigned integers where zero indicates 0, and 216 indicates 2π.

### 2.2.1 IHU to ADCS

The first byte represents the command ID.

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Byte Offset | 0x00 | 0x01 | 0x02 | 0x03 | 0x04 | 0x05 | 0x06 | 0x07 |
| 0x00 | 0x01: Request Orientation |  |  |  |  |  |  |  |

### 2.2.2 ADCS to IHU

ADCS replies with an array of three 16b unsigned integers.

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Byte  Offset | 0x00 | 0x01 | 0x02 | 0x03 | 0x04 | 0x05 | 0x06 | 0x07 |
| 0x00 | Roll Angle | | Pitch Angle | | Yaw Angle | |  |  |

## 2.3 Temperature Data Request

The temperatures are represented with an 8b signed integer with 1°C/LSB.

### 2.3.1 IHU to ADCS

The first byte represents the command ID.

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Byte  Offset | 0x00 | 0x01 | 0x02 | 0x03 | 0x04 | 0x05 | 0x06 | 0x07 |
| 0x00 | 0x02: Request Temperatures |  |  |  |  |  |  |  |

### 2.3.2 ADCS to IHU

The ADCS replies with an array of five 8b signed integers.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Byte  Offset | 0x00 | 0x01 | 0x02 | 0x03 |
| 0x00 | Coil X Driver Temperature | Coil Y Driver Temperature | Coil Z Driver Temperature | ADCS Temperature |
| 0x04 | GPS Temperature |  |  |  |

## 2.4 Coil Control Data Request

The PWM is represented by a 16b unsigned integer.

### 2.4.1 IHU to ADCS

The first byte represents the command ID.

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Byte  Offset | 0x00 | 0x01 | 0x02 | 0x03 | 0x04 | 0x05 | 0x06 | 0x07 |
| 0x00 | 0x03: Request PWM |  |  |  |  |  |  |  |

### 2.4.2 ADCS to IHU

The ADCS replies with an array of three 16b integers.

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Byte  Offset | 0x00 | 0x01 | 0x02 | 0x03 | 0x04 | 0x05 | 0x06 | 0x07 |
| 0x00 | Coil X Driver PWM Out | | Coil Y Driver PWM Out | | Coil Z Driver PWM Out | |  |  |

## 2.5 Coil Current Data Request

The current is represented by a 16b signed integer with 150µA/LSB.

### 2.5.1 IHU to ADCS

The first byte represents the command ID.

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Byte  Offset | 0x00 | 0x01 | 0x02 | 0x03 | 0x04 | 0x05 | 0x06 | 0x07 |
| 0x00 | 0x04: Request Coil Currents |  |  |  |  |  |  |  |

### 2.5.2 ADCS to IHU

The ADCS replies with an array of three 16b currents.

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Byte  Offset | 0x00 | 0x01 | 0x02 | 0x03 | 0x04 | 0x05 | 0x06 | 0x07 |
| 0x00 | Coil X Driver Current | | Coil Y Driver Current | | Coil Z Driver Current | |  |  |

## 2.6 Orientation Commands

These are the general rotation commands the satellite will use to orient itself when aiming towards a location on Earth, a point in space, to position solar panels, or to protect the satellite from temperature related damage.

### 2.6.1 IHU to ADCS

The first byte is the CID, and all three parameters are angles, as defined in Section 2.2.

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Byte  Offset | 0x00 | 0x01 | 0x02 | 0x03 | 0x04 | 0x05 | 0x06 | 0x07 |
| 0x00 | 0x05: Adjust Orientation | Roll | | Pitch | | Yaw | |  |

### 2.6.2ADCS to IHU

The ADCS replies with an error code defined in Code SOP 6.4.1.

## 2.7 Satellite Maneuvers for Earth

This command passes in a latitude and a longitude as two 32b signed integers to find and maintain a fixed direction towards a location on Earth. This will point the selected piece of the satellite towards the given parameters around the Earth.

### 2.7.1 IHU to ADCS

The first byte is the CID, and both remaining parameters are the respective geographic coordinates, as defined in Section 2.1.

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Byte  Offset | 0x00 | 0x01 | 0x02 | 0x03 | 0x04 | 0x05 | 0x06 | 0x07 |
| 0x00 | 0x06: Point Camera  0x07: Point Antenna | Latitude | | | | Longitude | | |
| 0x08 | Longitude |  |  |  |  |  |  |  |

### 2.7.2 ADCS to IHU

The ADCS replies with an error code defined in Code SOP 6.4.1.

## 2.8 Satellite Maneuvers for Space

This command will pass in an 8b unsigned integer representing the face, a 32b unsigned representing the declination in arcseconds, and a 32b unsigned integer representing Right Ascension in seconds. For more information about the Equatorial Coordinate System, please go to [Wikipedia’s page](https://en.wikipedia.org/wiki/Equatorial_coordinate_system) on the subject.

### 2.8.1 IHU to ADCS

The first byte is the CID, the parameters are the respective equatorial coordinates.

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Byte  Offset | 0x00 | 0x01 | 0x02 | 0x03 | 0x04 | 0x05 | 0x06 | 0x07 |
| 0x00 | 0x07: Point Camera  0x08: Point Solar Panels | Right Ascension | | | | Declination | | |
| 0x08 | Declination |  |  |  |  |  |  |  |

### 2.8.2 ADCS to IHU

The ADCS replies with an error code defined in Code SOP 6.4.1.

## 2.9 Roast the Chicken

These functions are primarily for maintaining the health of the satellite. The function “Roast the Chicken” behaves similarly to a rotisserie, evenly distributing the received power from the sun, aiding to normalize temperatures. As it is used to remedy a temperature related issue, it will take precedence, and does not need to be enqueued. It will, instead, become the immediate action until temperature levels are normalized or a new command is sent.

### 2.9.1 IHU to ADCS

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Byte  Offset | 0x00 | 0x01 | 0x02 | 0x03 | 0x04 | 0x05 | 0x06 | 0x07 |
| 0x00 | 0x09: Roast the Chicken |  |  |  |  |  |  |  |

### 2.9.2 ADCS to IHU

The ADCS replied with an error code, defined in Code SOP 6.4.1, indicating the satellite is now executing the maneuver “Roast the Chicken”.

## 2.10 Drift

The drifting command halts the work of the ADCS’s X, Y, and Z coils, and lets it tumble freely.

### 2.10.1 IHU to ADCS

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Byte  Offset | 0x00 | 0x01 | 0x02 | 0x03 | 0x04 | 0x05 | 0x06 | 0x07 |
| 0x00 | 0x10: Drift |  |  |  |  |  |  |  |

### 2.10.2 ADCS to IHU

The ADCS replies with an error code defined in Code SOP 6.4.1.

# 3 Example Communication

## 3.1 Simple Data Request for Location

IHU: [0xAC]0x00 [ADCS write] location request

ADCS collects location data and stores array in its buffer

IHU: [0xAD] [ADCS read]

ADCS: 0xBFEC 0.0000, 0.000

## 3.2 Simple Repeated Data Request

IHU: [0xAC]0x02 [ADCS write] temperature request

IHU: [0xAC]0x00 [ADCS write] location request

ADCS collects location data and stores array in its buffer

IHU: [0xAD] [ADCS read]

ADCS: 0xBFEC 0.000, 0.100

1. [Geographic Coordinate System](https://en.wikipedia.org/wiki/Geographic_coordinate_system) [↑](#endnote-ref-1)